# MI_GetCartridgeRomCycle2nd

## C Specification

  `#include <nitro/mi.h>`
  `MICartridgeRomCycle2nd MI_GetCartridgeRomCycle2nd( void )`

## Description

Gets the setting for the 2nd access cycle to the Game Pak's ROM region.

The returned values are in the form of `MICartridgeRomCycle2nd`. The meanings are shown below.

`MI_CTRDG_ROMCYCLE2_4` | 4 cycles
`MI_CTRDG_ROMCYCLE2_6` | 6 cycles

## Arguments

None.

## Return Values

The setting for the 2nd access cycle to the Game Pak's ROM region.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRomCycle1st, MI_SetCartridgeRomCycle2nd, MI_GetCartridgeRomCycle1st`

## Revision History

07/01/2004 Name changed from "2" to "2nd"
05/25/2004 Added "cartridge" to "name"
12/18/2003 Initial version