# GX_VCountEqIntr

## Syntax

      #include <nitro/gx/gx.h>

      void GX_VCountEqIntr(BOOL enable);

## Arguments

enable | Specifies whether to issue interrupt request when value is equal to the V-counter value.

## Returned value

None

## Explanation

If the argument is TRUE, an interrupt request is issued when the set value is equal to the V-counter. If the argument is FALSE, an interrupt request is not issued.

The function name has been changed from `GX_VCounterEqIntr` to `GX_VCountEqIntr`. For compatibility, `GX_VCountEqIntr` has been defined with a separate name from `GX_VCounterEqIntr`.

## See also:

`GX_IsVCountEq`, `GX_SetVCountEqVal`

## History

01/19/2004 Initial Version
10/19/2004 Name changed from `GX_VCounterEqIntr` to `GX_VCountEqIntr`