PAD Demos

# PAD Sample Demos

## Location

`$NitroSDK/build/demos/pad`

## Compilation

Move to the `$NitroSDK/build/demos/pad` directory and enter:

> `% make`

The executable files (`*.nef` and `*.srl`) will be generated in `$NitroSDK/build/demos/pad/sample_name/bin/platform/target/`.

For example, the path may be:

    $NitroSDK/build/demos/pad/padRead/bin/ARM9-TEG/Release/

## Execution

Navigate to the `$NitroSDK/build/demos/pad/sample_name/bin/platform/target/` directory and perform one of the following:

- Execute `*.nef` and `*.srl` with ensata.
- Execute `*.srl` with the TEG version of the IS-NITRO-EMULATOR.
- Load and execute `*.nlf` with the IS-NITRO-DEBUGGER.
- Execute `*.srl` with the IS-NITRO-DEBUGGER.

## Description

`padRead` | Displays pad status.

## Operation

Works in all execution environments.

## See Also

PAD Function list

## Revision history

08/17/2004 Standardized the notation of the IS-NITRO-EMULATOR.
07/10/2004 Change from `.bin` to `.srl.`
01/09/2004 Initial version.