# NNS_G2dSetCellTransferStateRequested

## C Specification

      #include <nnsys/g2d/g2d_CellTransferManager.h>

      void NNS_G2dSetCellTransferStateRequested(
              u32     handle,
              u32     srcOffset,
      u32     szByte );

## Arguments

handle | [IN] Handle of cell VRAM transfer state object
srcOffset | [IN] Offset value from the start of the transfer source data
szByte | [IN] Transfer size

## Return Values

None.

## Description

Sets the cell VRAM transfer state object in the VRAM transfer request state. For the state object set in the VRAM transfer request state, a VRAM transfer is actually requested if `NNS_G2dUpdateCellTransferStateManager()` is checked and the "to be drawn" flag is valid.

## See Also

`NNS_G2dUpdateCellTransferStateManager
`

## Revision History

07/20/2004 Initial version.