WVR Demos

# Wireless Driver Operation Control Library (WVR) Sample Demo

## Location

`$NitroSDK/build/demos/wvr`

## Compilation

Move to the `$NitroSDK/build/demos/wvr` directory and enter

> `% make`

Executable (.`.nef`, `.srl`) files will be generated in

> ``$NitroSDK/build/demos/wvr/sample_name/bin/platform/target/``

For example:

> `$NitroSDK/build/demos/wvr/simple/bin/ARM9-TS/Release/`

## Execution

Move to the `$NitroSDK/build/demos/wvr/sample_name/bin/platform/target/` directory and perform one of the following:

- Load a `*.nlf` file with IS-NITRO-DEBUGGER and execute it
- Execute a `*.srl` file with IS-NITRO-DEBUGGER

## Description

`simple` | This is a simple sample that demonstrates communications using VRAM-D in wireless communications via the WVR library.
`switchover` | This is a sample that switches allocations for single VRAMs to rendering-use or communications-use. When the start button is pushed, the sample demos below will switch back and forth. `/build/demos/wvr/simple` `/build/demos/gx/UnitTours/Sub_Double3D`
`with_mb` | This is a sample used when the WVR library is in DS download play. It is based on the following sample: /build/demos/mb/multiboot-model

## Emulator

`The WVR demo does not work on ensata.`

## See Also

`List of WVR Functions`

## Revision History

02/17/2005 Initial version