# MB_TYPE_*

## Definitions

  `#include <nitro/mb.h>`

      /* boot type */
      #define	MB_TYPE_ILLEGAL		0	/* illegal state */
      #define	MB_TYPE_NORMAL		1	/* startup from ROM */
      #define	MB_TYPE_MULTIBOOT	2	/* multi-boot child */

## Description

The constant showing the startup state of the program. The meaning of each value is as follows. The meaning of each enumerator constant is shown in the following table:

Constant | Description
MB_TYPE_ILLEGAL | An illegal state; the startup state cannot be determined.
MB_TYPE_NORMAL | The normal startup state from a NITRO-CARD.
MB_TYPE_MULTIBOOT | The multi-boot startup state from a parent.

## See Also

`MBParam, MB_GetMultiBootParam, MB_IsMultiBootChild, MB_GetMultiBootParentBssDesc`

## Revision History

08/09/2004 Initial version.