# G3X_GetClipMtx

## C Specification

      #include <nitro/gx/g3x.h>

      s32 G3X_GetClipMtx(MtxFx44 * m);

## Arguments

`m` | Pointer to matrix in which the results have been substituted

## Return Values

Returns a value of "0" to indicate that the data acquisition is complete; returns a non-zero value to indicate that the geometry engine is busy.

## Description

If the return value is 0, the current clip coordinate matrix has been substituted in `*``m`. If the return value is not 0, the data cannot be obtain because the geometry engine is busy.

## See Also

## Revision History

01/19/2004 Initial version