# WMBssDesc

## Definitions

  `#include <nitro/wm.h>`

      typedef struct WMBssDesc
      {
      u16         length;
      u16         rssi;
      u8          bssid[ WM_SIZE_BSSID ];
      u16         ssidLength;
      u8          ssid[WM_SIZE_SSID];
      u16         capaInfo;
      struct
          {
      u16     basic;
      u16     support;
      } rateSet;
      u16         beaconPeriod;
      u16         dtimPeriod;
      u16         channel;
      u16         cfpPeriod;
      u16         cfpMaxDuration;
      u16         gameInfoLength;
      u16         rsv;
      WMGameInfo  gameInfo;
      } WMBssDesc;

## Elements

length | The size, in half word (`u16`) units, of available data stored in this whole structure.
bssid | Parent BSS ID. This value is parent MAC address and is unique to each device.
gameInfoLength | The available data byte amount stored in `gameInfo`.
gameInfo | The `WMGameInfo` structure storing specified parent information.
rssi `<–|` Used internally by library | Used internally in the library.
ssidLength
ssid
capaInfo
rateSet
beaconPeriod
dtimPeriod
channel
cfpPeriod
cfpMaxDuration
rsv

## Description

The structure stores information of parent discovered by result of search by `WM_StartScan` function.

## Revision History

10/06/2004 Initial version