WM Demos

# The Wireless Manager Sample Demo

## Location

`$NitroSDK/build/demos/wm`

## Compilation

Move to the `$NitroSDK/build/demos/wm` and enter

> `% make`

Executable (.`.nef`, `.srl`) files will be generated in

> ``$NitroSDK/build/demos/wm/sample_name/bin/platform/target/``

For example:

> `$NitroSDK/build/demos/wm/simple-1/bin/ARM9-TS/Release/`

## Execution

Move to the `$NitroSDK/build/demos/wm/sample_name/bin/platform/target/` directory and perform one of the following:

- Load a `*.nlf` file with IS-NITRO-DEBUGGER and execute it
- Load and execute `*.srl` files on the IS-NITRO-DEBUGGER.

## Description

`simple-1` | This is a simple feature sample that conducts communications with the MP protocol.
`dataShare-1` | This shares the game frame value by using the data sharing feature.
`ball` | This moves the OBJ by using the key sharing feature.
`dataShare-Model` | This demo has a large number of notes for the tutorial document.
`wep-1` | Demo that uses WEP for connection authentication during DS wireless play.

## Operation

As of 03/02/2005, this does not operate normally on ensata. On the standard IS-NITRO-EMULATOR hardware, only wired communications are supported. If you have purchased the wireless option, wireless operation is supported.

## See Also

`The WM Function List`

## Revision History

04/01/2005 Added `wep-1`
03/02/2005 Revised descriptions to reflect current support environment conditions.
08/17/2004 Initial Version