# RTC_GetTime

## C Specification

  `#include <nitro/rtc.h>`

      RTCResult RTC_GetTime( RTCTime* time );

## Arguments

time | Pointer to `RTCTime`, where time information will be stored.

## Return Values

If the request succeeds, it returns 0.
If the request fails, it returns some numeric value other than 0.

## Description

This function reads time data from the real time clock. It queries ARM7 for time data and returns the information once it is received. This is a synchronous version of `RTC_GetTimeAsync`.

## Caution

This function requires a PXI interrupt for synchronization. Do not call this function when PXI interrupts are prohibited.

## See Also

`RTC_GetTimeAsync, RTC_SetTime, RTC_SetTimeAsync, RTCResult, RTCTime`

## Revision History

03/08/2005 Standardized the Japanese term for "interrupt"
05/18/2004 Initial version