# SND_GetCaptureStatus

## C Specification

      #include <nitro/snd.h>

      u32 SND_GetCaptureStatus( void );

## Arguments

None.

## Return Values

This function uses a bit flag to indicate whether each sound capture is active. The return values indicate capture 0, capture 1 in order from the lower order bit. If the sound capture is active, the bit is set.

## Description

This function uses a return value to determine whether a sound capture is active.

### Caution

This function is carried out asynchronously with respect to ARM7 command functions. To acquire synchronization, you must use a function such as the `SND_IsFinishedCommandTag` function to confirm that the processing of ARM7 commands has completed.

## See Also

SND_IsFinishedCommandTag

## Revision History

08/10/2004 Initial version