MI_SetCartridgeRamAccessCycle

# MI_SetCartridgeRamCycle

## C Specification

  `#include <nitro/mi.h>`
  `void MI_SetCartridgeRamCycle( MICartridgeRamCycle c );`

## Arguments

c | Access cycle to access Game Pak's RAM region.

## Return Values

None.

## Description

Sets the access cycle for accessing the Game Pak's RAM region. Access cycles for the Game Pak's ROM region are set using `MI_SetCartridgeRomCycle1st` and `MI_SetCartridgeRomCycle2nd`.

The c argument is a `MICartridgeRamCycle` enumerate type. The meanings are shown below.

`MI_CTRDG_RAMCYCLE_6` | 6 cycles
`MI_CTRDG_RAMCYCLE_8` | 8 cycles
`MI_CTRDG_RAMCYCLE_10` | 10 cycles
`MI_CTRDG_RAMCYCLE_18` | 18 cycles

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_GetCartridgeRamCycle
MI_SetCartridgeRomCycle1st, MI_SetCartridegeRomCycle2nd
`

## Revision History

05/25/2004 Name changed by adding "cartridge." 12/18/2003 Initial version.