# MB_SetLifeTime

## C Specification

  `#include <nitro/mb.h>`
  `void MB_SetLifeTime(u16 tableNumber, u16 camLifeTime, u16 frameLifeTime, u16 mpLifeTime);`

## Arguments

tableNumber | CAM table number that sets the lifetime The default setting is 0xFFFF (all). The meaning of the argument is the same as that in `WM_SetLifeTime`.
camLifeTime | CAM table lifetime The default setting is 40 (4 seconds). The meaning of the argument is the same as that in `WM_SetLifeTime`.
frameLifeTime | The lifetime during infrastructure mode The default setting is 0xFFFF (unlimited). The meaning of the argument is the same as that in `WM_SetLifeTime`.
mpLifeTime | MP communication lifetime The default setting is 40 (4 seconds). The meaning of the argument is the same as that in `WM_SetLifeTime`.

## Return Values

None.

## Description

Specifies the various lifetimes for the WM library that is used internally in the MB library. The value specified by this function is used internally without modification as an argument in `WM_SetLifeTime`.
In a normal game application, the default setting is appropriate, so there is no need to call this function explicitly.
This function can only be called after `MB_Init` is called and before `MB_StartParent` is called.

## See Also

`MB_Init, MB_StartParent, WM_SetLifeTime`

## Revision History

04/11/2005 Initial version.