# MI_GetCartridgeRomCycle1st

## C Specification

  `#include <nitro/mi.h>`
  `MICartridgeRomCycle1st MI_GetCartridgeRomCycle1st( void );`

## Arguments

None.

## Return Values

The setting for the 1st access cycle to access the ROM cartridge.

## Description

Gets the setting for the 1st access cycle to access the ROM cartridge.

The returned values are in the form of `MICartridgeRomCycle1st`. The meanings are shown below.

`MI_CTRDG_ROMCYCLE1_6` | 6 cycles
`MI_CTRDG_ROMCYCLE1_8` | 8 cycles
`MI_CTRDG_ROMCYCLE1_10` | 10 cycles
`MI_CTRDG_ROMCYCLE1_18` | 18 cycles

`MI_SetAgbCartridgeFastestRomCycle` is used for settings when accessing an AGB Game Pak.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRomCycle1st, MI_SetCartridgeRomCycle2nd,
MI_GetCartridgeRomAccess2nd
MI_SetAgbCartridgeFastestRomCycle`

## Revision History

2005/02/10 Added description of `MI_SetAgbCartridgeFastestRomCycle`
07/01/2004 Name changed from "1" to "1st" 05/25/2004 Added "cartridge" to name 12/18/2003 Initial version.