# MB_CommBootRequest

## C Specification

  `#include <nitro/mb.h>`
  `BOOL MB_CommBootRequest( u16 child_aid );
  `

## Arguments

child_aid | The aid that indicates the child device that transmits the boot request

## Return Values

This function returns `TRUE` if the boot request was sent correctly to the specified child. Otherwise, it returns `FALSE`.

## Description

This function sends boot requests to a specific child performing multi-boot processing with the current parent.
This function returns `TRUE` if the notification of bootable state has already been received from the specific child, and if the boot request could be sent correctly to the specific child.

## See Also

`MBCommPState, MB_CommGetParentState, MB_CommGetChildUser, MB_StartParent, MB_End`

## Revision History

09/09/2004 Added argument.
08/11/2004 Initial version.