# MBParentBssDesc

## Definitions

  `#include <nitro/mb.h>`

      typedef	struct
      {
      u16         length;
      u16         rssi;
      u16    bssid[3];
      u16         ssidLength;
      u8              ssid[32];
      u16         capaInfo;
      struct
          {
      u16     basic;
      u16     support;
      } rateSet;
      u16         beaconPeriod;
      u16         dtimPeriod;
      u16         channel;
      u16         cfpPeriod;
      u16         cfpMaxDuration;
      } MBParentBssDesc;

## Description

The structure where parent information for the multi-boot child is saved.
This is the same as the part with `gameInfo` removed from the `WMbssDesc` structure. In `ssid[0]`, `ssid[1]`, `ssid[2]`, and `ssid[3]`, `GGID` that was set from the multiboot parent is stored in little-endian format. System can keep only one structure, which can be obtained with the `MB_GetMultiBootParentBssDesc` function.
Also, it is referenced internally when obtaining the connected parent information with the `MB_ReadMultiBootParentBssDesc` function.

## See Also

`MBGameRegistry`, `MB_GetMultiBootParentBssDesc`

## Revision History

11/02/2004 Matched the structure definition to the header file.
10/06/2004 Corrected links.
08/09/2004 Initial version.