# WMLinkLevel

## Definitions

  `#include <nitro/wm.h>`

      typedef enum WMLinkLevel
      {
      WM_LINK_LEVEL_0 = 0 ,
      WM_LINK_LEVEL_1 ,
      WM_LINK_LEVEL_2 ,
      WM_LINK_LEVEL_3

      } WMLinkLevel;

## Elements

WM_LINK_LEVEL_0 | The link strength is 0. This indicates that the radio state is noticeably bad, or is in an unlinked state.
WM_LINK_LEVEL_1 | The link strength is 1. This indicates that the radio state is comparatively bad.
WM_LINK_LEVEL_2 | The link strength is 2. This indicates that the radio state is comparatively good.
WM_LINK_LEVEL_3 | The link strength is 3. This indicates that the radio state is good.

## Description

This is a list type that indicates the link strength during wireless communications. The link strength is displayed in four steps, from 0 to 3. 0 indicates the lowest strength, or an unlinked state, while 3 indicates the highest strength and a good radio state.

## Revision History

08/25/2004 Initial version