# CARDBackupType

## Definition

  `#include <nitro/card.h>`
  `typedef enum {
  CARD_BACKUP_TYPE_EEPROM_4KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 9, 0),
  CARD_BACKUP_TYPE_EEPROM_64KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 13, 0),
  CARD_BACKUP_TYPE_EEPROM_512KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 16, 0),
  CARD_BACKUP_TYPE_FLASH_2MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 18, 0),
  CARD_BACKUP_TYPE_FLASH_4MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 19, 0),
  CARD_BACKUP_TYPE_FLASH_8MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 20, 0),
  CARD_BACKUP_TYPE_FRAM_256KBITS = CARD_BACKUP_TYPE_DEFINE(FRAM, 15, 0),
  CARD_BACKUP_TYPE_NOT_USE = 0
  } CARDBackupType;`

## Description

Indicates the enumerated constants that identify the backup device that is mounted in a NITRO-CARD.

## See Also

`CARD_IdentifyBackup CARD_GetCurrentBackupType`

## Revision History

04/05/2006 Added CARD_BACKUP_TYPE_FLASH_8MBITS
10/19/2005 Added CARD_BACKUP_TYPE_FLASH_4MBITS
07/11/2005 Added CARD_BACKUP_TYPE_FRAM_256KBITS
06/15/2005 Added CARD_BACKUP_TYPE_EEPROM_512KBITS
09/09/2004 Deleted CARD_BACKUP_TYPE_EEPROM_512KBITS, CARD_BACKUP_TYPE_EEPROM_1MBITS
08/23/2004 Changed enumeration value format, Added CARD_BACKUP_TYPE_FLASH_2MBITS
07/05/2004 Initial version

CONFIDENTIAL