# GX_HBlankIntr

## C Specification

      #include <nitro/gx/gx.h>

      s32 GX_HBlankIntr( BOOL enable );

## Arguments

enable | Sets whether to generate an H-Blank interrupt request

## Return Values

Returns the status of the H-Blank interrupt request generation enable flag before calling this function. When it is prohibited, a value of 0 is returned. When it is permitted, a value other than the value of 0 is returned.

## Description

When the argument is TRUE, this function generates an H-Blank interrupt. If it is `FALSE`, it does not generate one.

## See Also

`GX_IsHBlank`, `GX_VBlankIntr`

## Revision History

07/26/2004 Revised the description of the return values.
01/19/2004 Initial version.

CONFIDENTIAL