# GX_BeginLoadClearImage

## C Specification

      #include <nitro/gx/gx_load.h>

      void GX_BeginLoadClearImage(void);

## Arguments

None.

## Return Values

None.

## Description

This function should be called before transferring the clear image to the clear image slot. Internally, it allocates to LCDC the banks that were allocated to the clear image slot and prepares to DMA transfer the clear image using `GX_LoadClearImageColor` and `GX_LoadClearImageDepth`.

Note: VRAM banks must be allocated to the clear image slot using `GX_SetBankForClearImage` in advance.

## See Also

`GX_LoadClearImageColor`, `GX_LoadClearImageDepth`, `GX_EndLoadClearImage`

## Revision History

02/09/2004

- Revised and expanded the description

01/19/2004 Initial version

CONFIDENTIAL