CTRDG Demos

# Rumble Pak Sample Demo

## Location

`$NitroSDK/build/demos/vib`

## Compilation

Move to the `$NitroSDK/build/demos/vib` directory and enter

> `% make`

Executable (`.nef`, `.srl`) files will be generated in

> `$NitroSDK/build/demos/vib/(sample_name)/bin/(platform)/(target)/`

For example:

> `$NitroSDK/build/demos/vib/pulse_vib/bin/ARM9-TS/Release/`

## Execution

First, plug in the Rumble Pack used as an option Game Pak for the NintendoDS into the IS-NITRO-EMULATOR.

Move to the `$NitroSDK/build/demos/vib/sample_name/bin/platform/target/` directory and perform one of the following:

- Load and execute a `*.nlf` file with IS-NITRO-DEBUGGER.
- Execute a `*.srl` file with IS-NITRO-DEBUGGER.

## Description

`pulse_vib` | Sample that allows any pulse to be generated for the Rumble Pak.

## Operation

`pulse_vib does not work properly with ensata.`

## See Also

List of Rumble Pak (VIB) API Functions

## Revision History

03/02/2006 Initial version.

CONFIDENTIAL