MB_Init

# MB_ReadMultiBootParentBssDesc

## C Specification

  `#include <nitro/mb.h>`
  `void MB_ReadMultiBootParentBssDesc(WMBssDesc *p_desc,
  u16 parent_max_size, u16 child_max_size, BOOL ks_flag, BOOL cs_flag);`

## Arguments

p_desc | pointer to `WMBssDesc` structure storing parent information
parent_max_size | maximum send size of MP parent that the connected parent sets by the `WM_SetParentParameter` function. This size must be stipulated and specified with the application beforehand.
child_max_size | maximum send size of MP child that the connected parent sets by the `WM_SetParentParameter` function. This size must be stipulated and specified with the application beforehand.
ks_flag | key sharing setting flag that the connected parent sets by the `WM_SetParentParameter` function. This setting must be stipulated and specified with the application beforehand.
cs_flag | continuous send setting flag that the connected parent sets by the `WM_SetParentParameter` function. This setting must be stipulated and specified with the application beforehand.

## Return Values

None.

## Description

If called by a multiboot child, this function stores information for connection to specified memory based on parent information retrieved with the `MB_GetMultiBootParentBssDesc` function. The `WMBssDesc` structure stored by this function can be handled the same as parent information retrieved with the `WM_StartScan` function, and can be provided in an argument of the `WM_StartConnect` function.

## See Also

WM_SetParentParameter, `WM_StartScan`, `WM_StartConnect`, `MB_GetMultiBootParentBssDesc`

## Revision History

10/05/2004 Initial version.

CONFIDENTIAL