CARD_IsEnabled

# CARD_Enable

## C Specification

  `#include <nitro/card.h>`
  `void CARD_Enable(BOOL enable);`

## Arguments

enable | Configures permission to access NITRO-CARD `TRUE` sets state to permit access; `FALSE` sets state to prohibit access.

## Return Values

None.

## Description

Changes the state, enabling or disabling access to NITRO-CARD. If the state prohibits access to NITRO-CARD, the program will forcedly halt when NITRO-CARD is accessed.
Access is prohibited in the initial state of a child program that has started from a wireless download.

## Note

If you are going to use this function to enable access to NITRO-CARD, be sure to follow the stipulations in the Programming Guideline. Confirm that the procedure is correct before calling the function.

## See Also

`CARD_Init`, `CARD_IsEnabled`

## Revision History

12/15/2004 Initial version.

CONFIDENTIAL