# GX_SetVCount

## C Specification

      #include <nitro/gx/gx.h>

      void GX_SetVCount(s32 count);

## Arguments

`count` | V-Count to set in the V-Counter (202 ≤ `count` ≤ 212)

## Return Values

None.

## Description

This function writes a value in the V-Count register. The written value takes effect when the V-Counter is updated. First confirm that the current V-Count is 202 – 212. Then write a value that is between 202 – 212.

## See Also

GX_GetVCount

## Revision History

01/19/2004 Initial version

CONFIDENTIAL