CHT Demos

# Pictochat Library (CHT) Demos

## Location

`$NitroSDK/build/demos/cht`

## Compilation

Move to the `$NitroSDK/build/demos/card` and input

> `% make`

Executable (.`.nef`, `.srl`) files will be generated in

> `$NitroSDK/build/demos/cht/sample_name/bin/platform/target/`

For example:

> `$NitroSDK/build/demos/cht/catch-1/bin/ARM9-TS/Release/`

## Execution

Move to the`$NitroSDK/build/demos/cht/sample_name/bin/platform/target/` directory, and do one of the following.

- Load and execute a `*.nlf` file with IS-NITRO-DEBUGGER.
- Execute a `*.srl` file with IS-NITRO-DEBUGGER

## Description

`catch-1` | This demo uses the Pictochat search feature to detect the Pictochat parent's beacon. It uses the WH sample module in `$NitroSDK/build/demos/wireless_shared/wh` for wireless control.
`catch-2` | This demo uses the Pictochat search feature to detect the Pictochat parent's beacon. It uses the WC sample module in `$NitroSDK/build/demos/wireless_shared/wc` for wireless control.
`catch-min` | This demo uses the Pictocatch feature to detect the beacon of the Pictochat parent. Wireless control does not use the special sample module. Rather, it uses a unique implentation of the miniumum functionality.

## Emulator

`The CHT library demos will not work with ensata.`

## See Also

`CHT function list`

## Revision History

07/14/2005 Added catch-min
05/10/2005 Initial Version

CONFIDENTIAL