# GX_VCountEqIntr

## C Specification

      #include <nitro/gx/gx.h>

      void GX_VCountEqIntr(BOOL enable);

## Arguments

enable | Specifies whether to issue interrupt request when value is equal to the V-counter value.

## Return Values

None.

## Description

If the argument is TRUE, an interrupt request is issued when the set value is equal to the V-counter. If it is `FALSE`, it does not generate one.

The function name has been changed from `GX_VCounterEqIntr` to `GX_VCountEqIntr`. For compatibility, `GX_VCountEqIntr` has been defined with a separate name from `GX_VCounterEqIntr`.

## See Also

`GX_IsVCountEq`, `GX_SetVCountEqVal`

## Revision History

10/19/2004 Name changed from `GX_VCounterEqIntr` to `GX_VCountEqIntr`.
01/19/2004 Initial version.

CONFIDENTIAL