CTRDG_Read

# CTRDG_ReadAgbSram

## C Specification

      #include <nitro/ctrdg.h>

      void CTRDG_ReadAgbSram(u32 src, void* dst, u32 size);

      Corresponding AGB function: void ReadSram(u8 *src,u8 *dst,u32 size)

## Arguments

src | Source SRAM address to read (address on the AGB memory map).
dst | The address of the work area to store data that was read (address on the AGB memory map).
size | The size of data read in bytes.

## Return Values

None.

## Description

Reads data of the size given by "size" into the destination address given by "dst" from the SRAM address specified by argument.

The access cycle setting is created in the function and does not need to be set beforehand.

Note: The cartridge bus is locked for a set period by this function.
Note that the AGB backup device cannot be accessed normally with version IS-NITRO-DEBUGGER 1.66 or earlier.

## See Also

`CTRDG_ReadAgbSramAsync
`

## Revision History

05/25/2006 Added a description that the AGB backup device cannot be accessed normally with version IS-NITRO-DEBUGGER 1.66 or earlier.
04/07/2006 Initial version.

CONFIDENTIAL