# WM_CopyBssid

## C Specification

      #include <nitro/wm/ARM9/wm_api.h>

      static inline
      void WM_CopyBssid( const u8* src , u8* dst );
      static inline
      void WM_CopyBssid16( const u8* src , u8* dst );

## Arguments

``src`` | Designates the pointer to the BSSID of the copy source. With `WM_CopyBssid16`, this address must be aligned to a 16-bit boundary.
`dst` | Designates the pointer to the BSSID of the copy destination. With `WM_CopyBssid16`, this address must be aligned to a 16-bit boundary.

## Return Values

None.

## Description

Copies the BSSID. `WM_CopyBssid16` can be used only if both compared addresses are aligned to 16-bit boundaries. This will improve performance somewhat.

## See Also

`WM_IsBssidEqual, WM_IsBssidEqual16`

## Revision History

02/10/2005 Added `WM_IsBssidEqual16`
11/10/2004 Initial version.

CONFIDENTIAL