PAD Demos

# PAD Sample Demos

## Location

`$NitroSDK/build/demos/pad`

## Compilation

Move to the `$NitroSDK/build/demos/pad` directory and enter

> `% make`

Executable (.`.nef`, `.srl`) files will be generated in

> `$NitroSDK/build/demos/pad/sample_name/bin/platform/target/`

For example:

> `$NitroSDK/build/demos/pad/padRead/bin/ARM9-TS/Release/`

## Execution

Navigate to the `$NitroSDK/build/demos/pad/sample_name/bin/platform/target/` directory and perform one of the following:

- Execute `*.nef`, `*.srl` with ensata.
- Load a `*.nlf` file with IS-NITRO-DEBUGGER and execute it
- Execute a `*.srl` file with IS-NITRO-DEBUGGER

## Description

`padRead` | Displays pad status.

## Emulator

`Works in all execution environments.`

## See Also

`PAD Function list`

## Revision History

03/02/2005 Revised descriptions to reflect current support environment conditions.
08/17/2004 Standardized the notation of the IS-NITRO-EMULATOR.
07/10/2004 Change from `.bin` to `.srl.`
01/09/2004 Initial Version

CONFIDENTIAL