----------------------------------------------------------------------------
  OPTPiX(R) iMageStudio(R) 5

  Hardware Key Manual

      Copyright(C) 1997-2004 web technology Corp. All rights reserved.
----------------------------------------------------------------------------

Thank you for choosing OPTPiX iMageStudio.
To use iMageStudio, you need to set up a Hardware Key properly. 
This document gives you information for setting up the Hardware Key.

Please consult the corresponding sections to your hardware key type:
Parallel Port (PP: Step 1, 2, 4, 5, 7, 8, 9, and 10) or
USB (USB: Step 2, 3, 4, 5, 6, 7, 8, 9, and 10).

  * USB hardware key is not available for Windows NT 4.0.


-----------------------------------------------------------
1. Install Parallel Port Hardware Key to Your Computer (PP)
-----------------------------------------------------------

    i. Find a Parallel Port Hardware Key for iMageStudio.
       Plug it to the parallel port of the PC on which you are to
       run iMageStudio.

   ii. Plug the Hardware Key to D-Sub25pin parallel port.
       The parallel port must be configured as "Normal" or "Bidirectional"
       in the BIOS SETUP of the PC. The Key may not work if the port is
       set in ECP or EPP.

  iii. Make sure to plug the Hardware Key directly to the parallel port. 
       Any device should not be placed between the Hardware Key and the
       parallel port; the Hardware Key may not work correctly.

  * The parallel port hardware key and the USB hardware key do not function
    at the same time.


-------------------------------
2. Install iMageStudio (PP/USB)
-------------------------------

  Install iMageStudio using its installer CD-ROM. And input the
  Registration Key Number, which is described on the License Agreement.


--------------------------------------------------
3. Install USB Hardware Key to Your Computer (USB)
--------------------------------------------------

    i. Log in as "Administrator" or a member of "Administrators Group"
       if your PC is Windows 2000/XP.

   ii. Restart your PC after the installation of iMageStudio.
       Then, plug the USB Hardware Key.

  iii. The hardware key "Aladdin USB Key" will be recognized and its driver
       will be automatically installed.

   iv. If the Plug & Play process did not finish properly, follow the steps
       below.

         1) In Control Panel: double-click "System", select "Hardware" tab,
            and click "Device Manager".
         2) Double-click "Universal Serial Bus controllers".
         3) If you found "?" mark on Aladdin device, delete the device.
         4) Close Control Panel and restart your PC.

    v. If the hardware key is still recognized as "Unknown Device", install
       the driver manually from Device Manager.
       The driver file (AKSUSB.INF)is in the following folder.

         If the OS installed in "C:\" drive:
             C:\WINNT\INF\ (for Windows 2000)
             C:\WINDOWS\INF\ (for Windows 98/ME/XP)

  * The parallel port hardware key and the USB hardware key do not function
    at the same time.


---------------------------------
4. Launching iMageStudio (PP/USB)
---------------------------------

  If any problems exist on the Hardware Key, iMageStudio will fail to start
  and error dialogs will appear.
  Here are the possible error messages and their solutions.

 +- Message
 |    Some required drivers  for start up may not be correctly installed.
 |    Please check your system, uninstall the program, and reinstall
 |    from the original CD-ROM.
 |
 |
 +- Reason and solution
      The Hardware Key driver version is old or not installed.
      Please reinstall iMageStudio or install Hardware Key manually.


 +- Message
 |    Hardware key not found.
 |    Please check 'Bad connection', 'Invalid hardware key ' etc.
 |
 |
 +- Reason and solution
      iMageStudio could not found the Hardware Key.

      For Parallel Port Hardware Key, check whether the hardware key
      is correctly plugged to the parallel port of your PC,
      and the parallel port should be configured as
      "Bidirectional" in BIOS SETUP.

      If using USB hardware key, the hardware key is not properly plugged
      to the USB port, or the setting of USB port may have problem(s).
      Check the USB hardware key whether the hardware key is correctly
      plugged to the USB port of your PC.  Or deselect "Disable"
      for USB port in BIOS SETUP.


 +- Message
 |    Hardware key cannot be recognized.
 |    Please check 'Bad connection', 'Invalid hardware key ' etc.
 |
 |
 +- Reason and solution
      iMageStudio recognized a Hardware Key but not for the version of
      iMageStudio you try to start.
      Please replace the Hardware Key with one for iMageStudio 4.


-----------------------------------
5. HASP Diagnostic Utility (PP/USB)
-----------------------------------

  "HASP Diagnostic Utility" is a utility program to check all information
  about the HASP of your computer system. 
  You can save the report made by this utility in your disk.

  HASP Diagnostic Utility is at "ETC\HASPDIAG" folder in the iMageStudio's
  installer CD-ROM.  Launch "DIAGNOSTIX.EXE" in "HASPDIAG" folder.

  * iMageStudio User Support will not be applied to any problem occurred
    using this program.


-------------------------------
6. Intel USB System Check (USB)
-------------------------------

  i.  "Intel USB System Check" is the tool for checking the system
      information related to USB.

  ii. This tool is "USBREADY.EXE" of \Etc\Haspdiag\ folder in the CD-ROM.

  * iMageStudio User Support will not be applied to any problem occurred
    using this program.


------------------------------
7. About Windows 2000 (PP/USB)
------------------------------

  Notice on followings about Windows 2000.

  i.  Reinstall iMageStudio when you upgrade from Windows 95/98 to
      Windows 2000. Each operating system requires different driver for
      the Hardware Key.

  ii. Reinstallation of iMageStudio is not necessary for upgrading from
      Windows NT4.0 to Windows 2000.


----------------------------
8. About Windows XP (PP/USB)
----------------------------

  Reinstall iMageStudio when you upgrade from Windows 98/ME/NT4.0/2000 to
  Windows XP. Each operating system requires different driver for
  the Hardware Key.


------------------------------------------------------------------
9. If Hardware Key Driver is already installed in your PC (PP/USB)
------------------------------------------------------------------

  The latest version of the hardware key driver is in the iMageStudio
  CD-ROM. By installation of iMageStudio, the hardware key driver should be
  upgraded to the latest version.

  However, the automatic upgrading may not be properly done in some cases.
  If the case has happened to your PC, once uninstall iMageStudio and
  reinstall iMageStudio.

    The version of the hardware key driver to be installed:

        HASP Hardware Key Driver 4.95

  * You can check the version by using HASP Diagnostic Utility.


-------------------------------------------------------------
10. Install/Uninstall a Hardware Key Driver Manually (PP/USB)
-------------------------------------------------------------

  Usually the driver software of the Hardware Key is installed/uninstalled
  automatically with iMageStudio, and you do not need to install/uninstall
  the driver manually.

  However, you may be required to install/uninstall the driver software
  alone.

    Steps for Manual Operations:

    a) Install the Driver of a Hardware Key Manually

       i. Insert iMageStudio CD-ROM to your CD-ROM drive.

      ii. Start MS-DOS prompt and enter:

          E:
          cd \DATA\HINSTALL
          HINSTALL.EXE /i

          (Note: replace E: with your CD-ROM drive letter if necessary.)

          The result of installation will be displayed.

    b) Uninstall the Driver of a Hardware Key Manually

       i. Insert iMageStudio CD-ROM to your CD-ROM drive.

      ii. Start MS-DOS prompt and enter:

          E:
          cd \DATA\HINSTALL
          HINSTALL.EXE /r

          (Note: replace E: with your CD-ROM drive letter if necessary.)

          The result will be displayed.

    c) Check the Hardware Key Driver Version Information

       i. Insert iMageStudio CD-ROM to your CD-ROM drive.

      ii. Start MS-DOS prompt and enter:

          E:
          cd \DATA\HINSTALL
          HINSTALL.EXE /info

          (Note: replace E: with your CD-ROM drive letter if necessary.)

          The version information will be displayed.

  * You also can see the version of the driver by using HASP Diagnostic 
    Utility. (HASP Device Driver tab sheet is on its report: ver. 4.70)

=============================================================================
Web Technology Corp.
http://www.webtech.co.jp/eng/
Copyright(C) 1997-2004 web technology Corp.
=============================================================================

* OPTPiX, iMageStudio and web technology are registered trademarks of 
  Web Technology Corp.
* All other trademarks and registered trademarks are the sole property of
  their respective owners.

[End of TEXT]
