# CARD_IsExecutableOnNTR

## Syntax

  `#include <nitro/card.h>`
  `void CARD_IsExecutableOnNTR(const `CARDRomHeader` *header);`

## Arguments

header | Pointer to the buffer storing the ROM header information of the program to be evaluated

## Return Values

Returns `TRUE` if the program can be started in DS mode. If not, returns `FALSE`.

## Description

Determines from the ROM header information whether the program can be run in DS mode.
This function returns `TRUE` if the program is compatible with Nintendo DS and built in NITRO or HYBRID mode. If the program is only for Nintendo DSi and built in LIMITED mode, the function returns `FALSE`.

## See Also

`CARDRomHeader`

## Revision History

2008/11/27 Initial version.

CONFIDENTIAL