# WM_IsBssidEqual

## Syntax

      #include <nitro/wm/ARM9/wm_api.h>

      static inline
      BOOL WM_IsBssidEqual( const u8* idp1 , const u8* idp2 );

      static inline
      BOOL WM_IsBssidEqual16( const u8* idp1 , const u8* idp2 );

## Arguments

`idp1` | Pointer to a BSSID to compare. With `WM_IsBssidEqual16`, this address must be aligned to a 16-bit boundary.
`idp2` | Pointer to a BSSID to compare. With `WM_IsBssidEqual16`, this address must be aligned to a 16-bit boundary.

## Return Values

TRUE if the BSSIDs are identical; FALSE if they are not identical.

## Description

Compares two BSSIDs. `WM_IsBssidEqual16` can be used only if both compared addresses are aligned to 16-bit boundaries. This will improve performance somewhat.

## See Also

`WM_CopyBssid, WM_CopyBssid16`

## Revision History

2005/02/10 Added `WM_IsBssidEqual16`
2004/11/10 Initial version.

CONFIDENTIAL