# MI_GetCartridgeRomCycle2nd

## Syntax

  `#include <nitro/mi.h>`
  `MICartridgeRomCycle2nd MI_GetCartridgeRomCycle2nd( void )`

## Arguments

None.

## Return Values

The setting for the 2nd access cycle to access the Game Pak's ROM region.

## Description

Gets the setting for the 2nd access cycle to access the Game Pak's ROM region.

The returned values are in the form of `MICartridgeRomCycle2nd`. The meanings are shown below.

`MI_CTRDG_ROMCYCLE2_4` | 4 cycles
`MI_CTRDG_ROMCYCLE2_6` | 6 cycles

`MI_SetAgbCartridgeFastestRomCycle` is used for settings when accessing an AGB Game Pak.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRomCycle1st,
MI_SetCartridgeRomCycle2nd, MI_SetCartridgeRomCycle2nd
MI_SetAgbCartridgeFastestRomCycle`

## Revision History

2005/02/10 Added description of `MI_SetAgbCartridgeFastestRomCycle.`
2004/07/01 Name changed from "2" to "2nd" 2004/05/25 Added "cartridge" to "name."
2003/12/18 Initial version.

CONFIDENTIAL