# MI_GetCartridgeRamCycle

## Syntax

  `#include <nitro/mi.h>`
  `MICartridgeRamCycle MI_GetCartridgeRamCycle( void )`

## Arguments

None.

## Return Values

Access cycle setting to access the cartridge RAM region

## Description

Gets the access cycle value settting for accessing the Game Pak's RAM region.

The return values are `MICartridgeRamCycle` enumerated types. The meanings are shown below.

`MI_CTRDG_RAMCYCLE_6` | 6 cycles
`MI_CTRDG_RAMCYCLE_8` | 8 cycles
`MI_CTRDG_RAMCYCLE_10` | 10 cycles
`MI_CTRDG_RAMCYCLE_18` | 18 cycles

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRamCycle,
MI_GetCartridgeRomCycle1st, MI_GetCartridgeRomCycle2nd
`

## Revision History

2004/05/25 Name changed by adding "cartridge." 2003/12/18 Initial version.

CONFIDENTIAL