# SCFG_IsNDmaAccessible

## Syntax

      #include <twl/scfg.h>

      inline BOOL SCFG_IsNDmaAccessible( void );

## Arguments

None.

## Return Values

If `TRUE`, the new DMA block is accessible.
If `FALSE`, the new DMA block is not accessible.

## Description

Determines if the new DMA block is configured to be accessible from the AHB.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be invoked on NITRO hardware.

## See Also

SCFG Overview
`SCFG_SetNDmaAccessible`

## Revision History

2007/10/03 Initial version.

CONFIDENTIAL