WVR Demos

# Wireless Driver Operation Control Library (WVR) Sample Demo

## Location

`$TwlSDK/build/demos/wvr`

## Compilation

Move to the `$TwlSDK/build/demos/wvr` directory and enter

> `% make`

Compiling will begin, and the SRL executable file and the NEF files with the binary information will be generated in `$TwlSDK/build/demos/wvr/(sample name)/bin/(platform)/(target)/`.

> ``

For example:

> `$TwlSDK/build/demos/wvr/simple/bin/ARM9-TS/Release/main.srl`

will be the executable file for the `simple` demo.

## Execution

### For NITRO ROMs:

If using IS-NITRO-DEBUGGER:

- Load and execute an NLF file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER
- Execute an SRL file with IS-NITRO-DEBUGGER using the `loadrun.exe` tool from a command line

If using IS-TWL-DEBUGGER:

- Load and execute an NLF file with IS-TWL-DEBUGGER.
- Execute an SRL file with IS-TWL-DEBUGGER
- Execute an SRL file with IS-TWL-DEBUGGER using the `loadrun.TWL.exe` tool from a command line

## Description

Name | Directories | Operation
--- | --- | ---
`simple` | `demos` | A simple sample that demonstrates communications using VRAM-D in wireless communications through the WVR library.
`switchover` | `demos` | A sample that switches allocations for single VRAMs to rendering use or communications use. When the start button is pressed, the sample demos below will switch back and forth. `/build/demos/wvr/simple` `/build/demos/gx/UnitTours/Sub_Double3D`
`with_mb` | `demos` | A sample used when the WVR library is in DS download play. It is based on the following sample: /build/demos/mb/multiboot-model

## Operation

The WVR library demos work properly only with NITRO ROM.

## See Also

List of WVR Functions

## Revision History

2008/07/11 Changed descriptions to support TWL.
2005/02/17 Initial version.

CONFIDENTIAL