# GX_SetVCountEqVal

## Syntax

      #include <nitro/gx/gx.h>

      void GX_SetVCountEqVal(s32 val);

## Arguments

val | The value to set for V-counter parity (0 ≤ `val` ≤ 262).

## Return Values

None.

## Description

This function configures the parity value that will be equal to the V-counter. The value must be an integer between 0 and 262.

To synchronize V-blanks during MP communications, the V-count value can roll back in a range of 202 to 210, so be careful when using this feature.

The name of this function has been changed from `GX_SetVCounterEqVal` to `GX_SetVCountEqVal`. For compatibility, `GX_SetVCounterEqVal` has been defined as another name for `GX_SetVCountEqVal`.

## See Also

`GX_GetVCountEqVal`, `GX_IsVCountEq`, `GX_VCountEqIntr`

## Revision History

2007/10/16 Added a note about use during MP communications.
2004/10/19 Changed the function name from `GX_SetVCounterEqVal` to `GX_SetVCountEqVal`.
2004/01/19 Initial version.

CONFIDENTIAL