# CAMERAIntrVsync

## Definition

  `#include <twl/camera.h>`

      typedef enum {
          CAMERA_INTR_VSYNC_NONE          = (0 << REG_CAM_CNT_IREQVS_SHIFT),
          CAMERA_INTR_VSYNC_NEGATIVE_EDGE = (2 << REG_CAM_CNT_IREQVS_SHIFT),
          CAMERA_INTR_VSYNC_POSITIVE_EDGE = (3 << REG_CAM_CNT_IREQVS_SHIFT)
      } CAMERAIntrVsync;

## Elements

CAMERA_INTR_VSYNC_NONE | Interrupts are disabled.
CAMERA_INTR_VSYNC_NEGATIVE_EDGE | Interrupts occur at the end of the camera VSync.
CAMERA_INTR_VSYNC_POSITIVE_EDGE | Interrupts occur at the start of the camera VSync.

## Description

This enumerated type is used to specify when camera VSync interrupts will occur.

## Revision History

2007/11/09 Initial version.

CONFIDENTIAL