SCFG_SetConfigBlockInAccessible

# SCFG_IsDSPReset

## Syntax

      #include <twl/scfg.h>

      static inline BOOL SCFG_IsDSReset( void );

## Arguments

None.

## Return Values

If `TRUE`, a reset signal is being sent to the DSP.
If `FALSE`, the reset signal has been canceled.

## Description

Gets the state of the reset signal being sent to the DSP block.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be called on NITRO hardware.

## See Also

SCFG Overview
`SCFG_ResetDSP`
`SCFG_ReleaseResetDSP`

## Revision History

2007/10/03 Initial version.

CONFIDENTIAL