# MB_CommBootRequest

## Syntax

  `#include <nitro/mb.h>`
  `BOOL MB_CommBootRequest( u16 child_aid );
  `

## Arguments

child_aid | The aid that indicates the child device that transmits the boot request

## Return Values

This function returns `TRUE` if the boot request was sent correctly to the specified child. Otherwise, it returns `FALSE`.

## Description

This function sends boot requests to a specific child performing multi-boot processing with the current parent.
This function returns `TRUE` if the notification of bootable state has already been received from the specific child, and if the boot request could be sent correctly to the specific child.

## See Also

`MBCommPState, MB_CommGetParentState, MB_CommGetChildUser, MB_StartParent, MB_End`

## Revision History

2004/09/09 Added argument.
2004/08/11 Initial version.

CONFIDENTIAL