# SCFG_IsCameraCKIClockEnable

## Syntax

      #include <twl/scfg.h>

      static inline BOOL SCFG_IsCameraCKIClockEnable( void );

## Arguments

None.

## Return Values

Control flag for the CAM_CKI clock.
Enables `CAM_CKI` (16.67MHz output) if `TRUE`.
Disables `CAM_CKI` (output fixed Low) if `FALSE`.

## Description

Gets the current CAM_CKI clock setting for the camera.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be called on NITRO hardware.

## See Also

SCFG Overview
`SCFG_SetCameraCKIClock`

## Revision History

2007/09/04 Initial version.

CONFIDENTIAL