# MI_GetNDmaIntervalTimer

## Syntax

  `#include <twl/mi.h>`
  `u32 MI_GetNDmaIntervalTimer( u32 ndmaNo );`

## Arguments

ndmaNo | DMA number to get settings for (0-3).

## Return Values

Timer value of the block transfer interval timer.

## Description

Gets the value of the block transfer interval timer setting.

It gets the value of the block transfer interval timer setting for the new TWL DMA specified in ndmaNo.

## See Also

`MI_SetNDmaInterval
`

## Revision History

2007/09/07 Initial version.

CONFIDENTIAL