# CARDBackupType

## Definition

  `#include <nitro/card.h>`
  `typedef enum {
  CARD_BACKUP_TYPE_EEPROM_4KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 9, 0),
  CARD_BACKUP_TYPE_EEPROM_64KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 13, 0),
  CARD_BACKUP_TYPE_EEPROM_512KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 16, 0),
  CARD_BACKUP_TYPE_EEPROM_1MBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 17, 0),
  CARD_BACKUP_TYPE_FLASH_2MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 18, 0),
  CARD_BACKUP_TYPE_FLASH_4MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 19, 0),
  CARD_BACKUP_TYPE_FLASH_8MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 20, 0),
  CARD_BACKUP_TYPE_FLASH_16MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 21, 0),
  CARD_BACKUP_TYPE_FLASH_64MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 23, 0),
  CARD_BACKUP_TYPE_NOT_USE = 0
  } CARDBackupType;`

## Description

Indicates the enumerated constants that identify the backup device mounted in a NITRO-CARD.

## See Also

`CARD_IdentifyBackup`
`CARD_GetCurrentBackupType`

## Revision History

2008/11/27 Deleted `CARD_BACKUP_TYPE_FRAM_256KBITS` from the usable line numbers.
2008/10/21 Deleted `CARD_BACKUP_TYPE_FRAM_256KBITS`.
2008/10/21 Added `CARD_BACKUP_TYPE_EEPROM_1MBITS`.
2007/08/22 Added `CARD_BACKUP_TYPE_FLASH_64MBITS`.
2007/02/23 Added `CARD_BACKUP_TYPE_FLASH_16MBITS`.
2006/04/05 Added `CARD_BACKUP_TYPE_FLASH_8MBITS`.
2005/10/19 Added `CARD_BACKUP_TYPE_FLASH_4MBITS`.
2005/07/11 Added `CARD_BACKUP_TYPE_FRAM_256KBITS`.
2005/06/15 Added `CARD_BACKUP_TYPE_EEPROM_512KBITS`.
2004/09/09 Deleted `CARD_BACKUP_TYPE_EEPROM_512KBITS` and `CARD_BACKUP_TYPE_EEPROM_1MBITS`.
2004/08/23 Changed the format of the enumerator values and added `CARD_BACKUP_TYPE_FLASH_2MBITS`.
2004/07/05 Initial version.

CONFIDENTIAL