# WMLinkLevel

## Definition

  `#include <nitro/wm.h>`

      typedef enum WMLinkLevel
      {
          WM_LINK_LEVEL_0 = 0 ,
          WM_LINK_LEVEL_1 ,
          WM_LINK_LEVEL_2 ,
          WM_LINK_LEVEL_3
      } WMLinkLevel;

## Elements

`WM_LINK_LEVEL_0` | Link strength is 0. This indicates that the signal status is noticeably bad or is in an unlinked state.
`WM_LINK_LEVEL_1` | Link strength is 1. This indicates that the signal status is comparatively bad.
`WM_LINK_LEVEL_2` | Link strength is 2. This indicates that the signal status is comparatively good.
`WM_LINK_LEVEL_3` | Link strength is 3. This indicates that the signal status is good.

## Description

List type that indicates the link strength during wireless communications. The link strength is displayed in four steps, from 0 to 3. Zero indicates the lowest strength, or an unlinked state, and 3 indicates the highest strength and a good radio state.

## Revision History

2004/08/25 Initial version.

CONFIDENTIAL