# MI_StopAllDma

## Syntax

  `#include <nitro/mi.h>`
  `void MI_StopAllDma( void )`

## Arguments

None.

## Return Values

None.

## Description

Stops all DMA channels. (However, all DMA channels does not include the TWL's new DMA channels.)

This function calls the `MI_StopDma` function for DMA channels 0-3.

## See Also

`MI_StopDma
`

## Revision History

2008/09/11 Initial version.

CONFIDENTIAL