# MI_GetNDmaArbitramentMode

## Syntax

  `#include <twl/mi.h>`
  `u32 MI_GetNDmaArbitramentMode( void );`

## Arguments

None.

## Return Values

DMA arbitration method.
If `MI_NDMA_ARBITRAMENT_FIX`, the fixed method is used.
If `MI_NDMA_ARBITRAMENT_ROUND`, the round-robin method is used.

## Description

Gets the currently configured DMA arbitration method of the new TWL DMA.

## Internal Operation

Accesses the DMA_GCNT register.

## See Also

`MI_SetNDmaArbitrament`
`MI_GetNDmaArbitramentRoundRobinCycle`

## Revision History

2008/10/30 Corrected the function name.
2007/09/07 Initial version.

CONFIDENTIAL