# SND_ResetMasterPan

## Syntax

      #include <nitro/snd.h>

      void SND_ResetMasterPan( void );

## Arguments

None.

## Return Values

None.

## Description

Disables the master pan that was set using the `SND_SetMasterPan` function.

### Note

If this function is called while sound is being played, noise may be generated when the master pan is switched.

This function is an ARM7 reserved function. After this function is called, its processing will occur only after the command is issued with the `SND_FlushCommand` function.

If program execution must be synchronized with process completion, first use the `SND_GetCurrentCommandTag` function to obtain the command tag immediately after calling this function. Then, after the command is issued, use the command tag and call either the `SND_IsFinishedCommandTag` or `SND_WaitForCommandProc` function to confirm that processing has finished or to wait for it to complete.

## See Also

`SND_SetMasterPan, SND_FlushCommand, SND_GetCurrentCommandTag, SND_IsFinishedCommandTag, SND_WaitForCommandProc`

## Revision History

2004/10/05 Initial version.

CONFIDENTIAL