# SND_GetCaptureStatus

## Syntax

      #include <nitro/snd.h>

      u32 SND_GetCaptureStatus( void );

## Arguments

None.

## Return Values

This function uses a bit flag to indicate whether each sound capture is active. The return values indicate capture 0, capture 1 in order from the lower order bit. If the sound capture is active, the bit is set.

## Description

This function uses a return value to determine whether a sound capture is active.

### Note

This function is carried out asynchronously with respect to ARM7 command functions. To achieve synchronization, you must use a function such as `SND_IsFinishedCommandTag` to confirm that ARM7 commands have finished processing.

## See Also

SND_IsFinishedCommandTag

## Revision History

2004/08/10 Initial version.

CONFIDENTIAL