TCL Demos

# TCL Application Sample Demos

## Location

`$TwlSDK/build/demos.TWL/tcl`

## Compilation

Move to the `$TwlSDK/build/demos.TWL/tcl` directory and enter the following.

> `% make`

Compilation starts, and a TAD file in NAND application format is created in

> `$TwlSDK/build/demos.TWL/tcl/(sample_name)/bin/(platform)/(target)/`

For example:

> `$TwlSDK/build/demos.TWL/tcl/tcl-1/bin/ARM9-TS.LTD/Release/tcl_1.tad`

The above path shows the file used to import the `simple` demo.

## Execution

Perform either of the following procedures.

- Open a TAD file using the IS-TWL-DEBUGGER software, and then import and run it.
- Use `$TwlSDK/bin/ARM9-TS/Release/TwlNmenu.srl` to import and then run a TAD file that is stored on an SD Card.

## Description

Name | Directory | Operation
--- | --- | ---
`tcl-1` | `demos.TWL` | Sample for displaying or deleting photo data from the `photo` region.
`tcl-2` | `demos.TWL` | Sample for adding photo data to the `photo` region.

## Operation

These demos do not work properly with ensata.

## See Also

## Revision History

2009/04/13 Initial version.

CONFIDENTIAL