# SCFG_SupplyClockToCamera

## Syntax

      #include <twl/scfg.h>

      static inline void SCFG_SupplyClockToCamera( BOOL sw );

## Arguments

sw | If `TRUE`, a clock will be supplied to the camera interface block. If `FALSE`, a clock will no longer be supplied.

## Return Values

None.

## Description

Configures the clock supply to the camera interface block.

To be safe, stop the clock while the camera interface block is stopped.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be called on NITRO hardware.

## See Also

SCFG Overview
`SCFG_IsClockSuppliedToCamera`

## Revision History

2007/09/04 Initial version.

CONFIDENTIAL